FLOW/LEVEL/PRESSURE SOFTWARE - OPERATIONAL OVERVIEW

VISUALIZATION VIEW LEVEL

IN 1 mA – IN 2 FLOW

FLOW – RESET VOLUME – INF VOLUME

IN 1 mA – OUT mA 1

IN 2 FLOW – OUT mA 2

OUTPUT SETTINGS

SETTINGS

CALIBRATION

OUTPUTS

OPTIONS

VIEW DATA

SETTING INPUT mA

PRESSURE

MENU LEVEL

INPUT 1

LEVEL

VOLUME

VOLUME UNIT

INPUT 2\*

SET K-FACTOR VALUE

FLOW UNIT

IN-LINE ADJUSTMENT

INPUT 1

AUTO CALIBRATION DENSITY

CORRECTION FACTOR

INPUT 2\*

AUTO CALIBRATION

1 SSR

2 SSR

RELE’ 3

RELE’ 4

4-20 mA 1

4-20 mA 2

OUTPUT TEST

\* Not available if the 2 input is not activated

LANGUAGE

FILTER INPUT 1

FILTER INPUT 2

BACKLIGHT

CONTRAST

DECIMAL POINT INPUT 1

DECIMAL POINT INPUT 2

PASSWORD

OUTPUT ACTIVATION

DEFAULT DATI

UPGRADE FIRMWARE

SCALE VALUE

SIGNAL PROBE

OUTPUT ACTIVATION

RESET STATISTICS

TYPE VISUAL mA1

ADJUST INPUT 4mA1

ADJUST INPUT 20mA1

INPUT 1

FULL SCALE mA1